Petunjuk Penggunaan Rangkaian - Directions for Use

1. Struktur Folder - Folder Structure

Di dalam rangkaian ini tersedia folder 'New Scheme' dan dua folder 'Old Scheme' untuk mengganti warna skema dari rangkaian.
Untuk mengubah warna standar rangkaian yang menggunakan skema baru ke skema lama cukup copy dan paste semua file
yang ada di folder 'Old Scheme' ke folder 'Eksterior'.
Untuk melakukan hal sebaliknya juga mengikuti cara yang sama, akan tetapi file yang dicopy berasal dari folder
'New Scheme'.

This set includes 'New Scheme' and two 'Old Scheme' folders to change train color scheme. For changing the standard
color scheme (uses new color scheme) to old color scheme just copy and paste all files from the 'Old Scheme' folder.
If you prefer to use new color scheme after using the old one, just copy and paste all files from the 'New Scheme' folder to the 'Eksterior' folder.

2. Penggunaan di BVE 2/4 - Using in BVE 2/4

Rangkaian ini secara default hanya mendukung penggunaan untuk openBVE. Jika anda memiliki BVE 2/4 dan ingin menggunakan
rangkaian ini di program tersebut, ubahlah header yang bertuliskan 'OPENBVE' menjadi 'BVE2000000' setelah membuka file Train.dat.

This set is only support openBVE by default. If you have BVE 2/4 versions and want to use this set in those programs,
please change the header 'OPENBVE' to 'BVE2000000' after opening the 'Train.dat' file.

3. Penomoran - Numbering

Rangkaian ini menggunakan skema penomoran awal secara default (6188-6245-6176-6175-6242-6181). Untuk mengubahnya ke sistem penomoran
gabungan dengan rangkaian 6151F (6158-6157-6176-6175-6245-6181), cukup ganti/hapus file 'num.bmp' dan ubah nama file 'mixednum.bmp' menjadi
'num.bmp'. Untuk mengembalikannya ke keadaan standar, copy dan paste file 'num.bmp' dan 'mixednum.bmp' dari folder 'New Scheme' atau 'Old Scheme 2'
ke folder 'Eksterior'.

This set uses the standard numbering arrangement by default (6188-6245-6176-6175-6242-6181). To change it with the 6181F+6151F arrangement
numbering (6158-6157-6176-6175-6245-6181), just rename/delete 'num.bmp' file and rename the 'mixednum.bmp' to the 'num.bmp'. But if you're
prefer to roll back the numbering into the default arrangement, copy and paste 'num.bmp' and 'mixednum.bmp' from the 'New Scheme' or 'Old Scheme 2'
folder to the 'Eksterior' folder. 